#! /bin/bash

. /etc/init.d/functions

cd /etc/sysconfig/network-scripts
. ./network-functions

[ -f ../network ] && . ../network

CONFIG=${1}

source_config

# On hotplug events, just bring the virtual device up as if it's normal Ethernet
if [ -n "$IN_HOTPLUG" ]; then
    exec sh -x /etc/sysconfig/network-scripts/ifup-eth ${CONFIG} $2 
fi

start_panu()
{
    PANDARGS="--persist --pidfile=/run/pand-${DEVICE}.pid --ethernet=${DEVICE} --autozap"
    [ "${CACHE}" != "no" -a "${CACHE}" != "NO" ] && PANDARGS="${PANDARGS} --cache"
    if [ "${REMOTEBDADDR}" = "" ]; then
        PANDARGS="${PANDARGS} --search"
    else
        PANDARGS="${PANDARGS} --connect ${REMOTEBDADDR}"
    fi
    /usr/bin/pand ${PANDARGS}
}

start_nap()
{
    :
}

start_gn()
{
    :
}

case "$ROLE" in
PANU)
    start_panu
    ;;
NAP)
    start_nap
    ;;
GN)
    start_gn
    ;;
*)
    echo Unknown BNEP mode :$ROLE
    ;;
esac

