#! /bin/bash

. /etc/init.d/functions

cd /etc/sysconfig/network-scripts
. ./network-functions

[ -f ../network ] && . ../network

CONFIG=${1}

source_config

# On hotplug events, just bring the virtual device up as if it's normal Ethernet
if [ -n "$IN_HOTPLUG" ]; then
    exec /etc/sysconfig/network-scripts/ifdown-eth ${CONFIG} $2
fi

stop_panu()
{
    kill -TERM $(cat /run/pand-${DEVICE}.pid)
}

stop_nap()
{
    kill -TERM $(cat /run/pand-${DEVICE}.pid)
    /usr/bin/pand -K
}

stop_gn()
{
    :
}

case "$ROLE" in
PANU)
    stop_panu
    ;;
NAP)
    stop_nap
    ;;
GN)
    stop_gn
    ;;
*)
    echo Unknown BNEP mode :$ROLE
    ;;
esac

